Getting Started: Running the “Device – CDC – Basic Demo” demo

Required Hardware: 1

Configuration 1: PICDEM FS USB.. 1

Configuration 2: PIC18F87J50 PIM... 1

Configuration 3: Explorer 16. 1

Configuration 4: Low Pin Count USB Development Kit 2

Configuration 5: PIC24F Starter Kit 1. 2

Configuration 6: PIC18F46J50 Full Speed USB Demo Board. 2

Configuration 7: PIC32 USB Starter Board. 2

Configuration 8: PIC18F Starter Kit 2

Configuring the Hardware: 2

Configuration 1: PICDEM FS USB.. 2

Configuration 2: PIC18F87J50 PIM... 3

Configuration 3: Explorer 16. 3

Configuration 4: Low Pin Count USB Development Kit 6

Configuration 5: PIC24F Starter Kit 1. 6

Configuration 6: PIC18F46J50 Full Speed USB Demo Board. 6

Configuration 7: PIC32 USB Starter Board. 7

Configuration 8: PIC18F Starter Kit 7

Firmware. 7

Running the Demo. 8

Push Button. 10

Trademarks: 13

## Required Hardware:

To run this project, you will need one of the following sets of hardware:

### Configuration 1: PICDEM FS USB

PICDEM FS USB (DM163025)

### Configuration 2: PIC18F87J50 PIM

PIC18F87J50 Plug-In-Module (PIM) (MA180021)

### Configuration 3: Explorer 16

Explorer 16 (DM240001)

USB PICtail™ Plus Daughter Card (AC164131)

And one of the following PIMs

PIC24FJ256GB110 Plug-In-Module (PIM) (MA240014)

PIC32MX USB Plug-In-Module (PIM) (MA320002)

### Configuration 4: Low Pin Count USB Development Kit

Low Pin Count USB Development Kit with PICKit 2 Debugger/Programmer (DV164126) or without Debugger/Programmer (DM164127)

### Configuration 5: PIC24F Starter Kit 1

PIC24F Starter Kit 1 (DM240011)

### Configuration 6: PIC18F46J50 Full Speed USB Demo Board

PIC18F46J50 Full Speed USB Demo Board (MA180024)

### Configuration 7: PIC32 USB Starter Board

PIC32 USB Starter Board (DM320003)

### Configuration 8: PIC18F Starter Kit

PIC18F Starter Kit (DM180021)

## Configuring the Hardware:

This section describes how to set up the various configurations of hardware to run this demo.

Configuration 1: PICDEM FS USB

Configuration 2: PIC18F87J50 PIM + HPC Explorer

Configuration 3: Explorer 16

Configuration 4: Low Pin Count USB Development Kit

Configuration 5: PIC24F Starter Kit 1

Configuration 6: PIC18F46J50 Full Speed USB Demo Board

Configuration 7: PIC32 USB Starter Kit

Configuration 8: PIC18F Starter Kit

### Configuration 1: PICDEM FS USB

1) If using the PICDEM FS USB Demo Board, no hardware related configuration or jumper setting changes should be necessary. The demo board need only be programmed with appropriate firmware.

### Configuration 2: PIC18F87J50 PIM

1) Short JP4 on the PIC18F87J50 PIM. This allows the demo board to be powered through bus power.

2) Short JP1 such that the “R” and “U” options are shorted.

### Configuration 3: Explorer 16

1) Before attaching the PIM to the Explorer 16 board, insure that the processor selector switch (S2) is in the “PIM” position as seen in the image below.

2) Short the J7 jumper to the “PIC24” setting

3) Before connecting the PIM to the Explorer 16 board, remove all attached cables from both boards. Connect the PIM to the Explorer 16 board. Be careful when connecting the boards to insure that no pins are bent or damaged during the process. Also insure that the PIM is not shifted in any direction and that all of the headers are properly aligned.

3a) If using the PIC24FJ64GB004 PIM, please insure that the programming port switch is switched in the PGX1 direction.

4) On the USB PICTail Plus board, short jumper JP1. Remove all other shorts on the board.

5) Connect the USB PICTail Plus board to either of the female PICTail Plus connectors or on the card edge connector (J9) at the edge of the Explorer 16 board.

Note: When using the HID bootloader for PIC32, it is important to modify the procdefs.ld file to relocate the sections of code that will hold the bootloader and those sections that will hold the user application. Example modified procdefs.ld files have been provided with each project. This file is currently named “Procdefs.ld.boot”. When using the example project with the bootloader it is required to remove the “.boot” section of the file. This will allow MPLAB to use this file instead of the default linker file. Once the linker file is renamed, however, the project will no longer work without the bootloader. Please rename the file in order to get the project working again with PIC32.

### Configuration 4: Low Pin Count USB Development Kit

1) Short pins 2 and 3 of J14. Make sure J12 is left open.

### Configuration 5: PIC24F Starter Kit 1

The PIC24F Starter Kit does not require any hardware setup to run this demo. This demo does, however, require the user to change the default selected device in the project before compiling the demo.

1) Open the associated project file for C30

2) In MPLAB Select “Configure->Select Device”

3) In the device list box in the top left corner of that window, select “PIC24FJ256GB106”

### Configuration 6: PIC18F46J50 Full Speed USB Demo Board

1) Short JP3 to allow the board to be powered from the USB.

### Configuration 7: PIC32 USB Starter Board

No specific hardware configuration is required for this demo. Use the OTG cable provided with the starter kit to connect OTG connector J5 (on the bottom side of the starter kit) to the PC.

### Configuration 8: PIC18F Starter Kit

No specific hardware configuration is required for this demo.

Firmware:

To run this project, you will need to load the corresponding firmware into the devices. There are two methods available for loading the demos: Precompiled demos and source code projects.

Precompiled Demos are available in the “<Install Directory>\USB – Precompiled Demos” folders. Each demo should be prefaced with the hardware platform it is compiled for. Select the file that matches the hardware that you have and the demo that you want to run. For more information about how to load a precompiled project, please see the “Getting Started – Loading a precompiled demo” guide.

The source code for this demo is available in the “<Install Directory\USB Device – CDC – Basic Demo” directory. In this directory you will find all of the user level source and header files as well as project and workspace files for each of the hardware platforms. Find the project (*.mcp) or workspace (*.mcw) file that corresponds to the hardware platform you wish to test. Compile and program the demo code into the hardware platform. For more help on how to compile and program projects, please refer to the MPLAB® IDE help available through the help menu of MPLAB IDE (Help->Topics…->MPLAB IDE).

Please note that when using either the C30 or C32 demo projects you will be required to select the correct processor for the demo board.

1) Open the associated project file

2) In MPLAB Select “Configure->Select Device”

3) In the device list box in the top left corner of that window, select the desired device.

Running the Demo:

This demo allows the device to appear like a serial (COM) port to the host. In order to run this demo first compile and program the target device. Attach the device to the host. If the host is a PC and this is the first time you have plugged this device into the computer then you may be asked for a .inf file.

Select the “Install from a list or specific location (Advanced)” option. Point to the “<Install Directory>\USB Device - CDC – Basic Demo\inf\win2k_winxp” directory

Once the device is successfully installed, open up a terminal program, such as hyperterminal. Select the appropriate COM port. On most machines this will be COM5 or higher.

Once connected to the device, there are two ways to run this example project. Typing a key in the terminal window will result in the device echoing that key plus one. So if the user presses “a”, the device will echo “b”. If the pushbutton is pressed the device will echo “ – Button Pressed – “ to the terminal window.

Note: Some terminal programs, like hyperterminal, require users to click the disconnect button before removing the device from the computer. Failing to do so may result in having to close and open the program again in order to reconnect to the device.

### Push Button

PICDEM FS USB:

PIC18F87J50 PIM:

Explorer 16:

Low pin count USB development kit:

PIC24F Starter Kit 1:

The PIC24F Starter Kit 1 does not implement the pushbutton for these demos. This functionality is not present in this demo.

PIC18F46J50 Full Speed USB Demo Board:

PIC32 USB Starter Kit

PIC18 Starter Kit

## Trademarks:

The Microchip name and logo, the Microchip logo, MPLAB, and PIC are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

PICDEM and PICTail are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

Microsoft, Windows, and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.