!_TAG_FILE_FORMAT	2	/extended format; --format=1 will not append ;" to lines/
!_TAG_FILE_SORTED	1	/0=unsorted, 1=sorted, 2=foldcase/
!_TAG_PROGRAM_AUTHOR	Darren Hiebert	/dhiebert@users.sourceforge.net/
!_TAG_PROGRAM_NAME	Exuberant Ctags	//
!_TAG_PROGRAM_URL	http://ctags.sourceforge.net	/official site/
!_TAG_PROGRAM_VERSION	5.5.4	//
!_TAG_REVISION_NAME	MCHPTags	//
!_TAG_REVISION_VERSION	6.0.1	//
AcquireTemperature	D:\LX-100PIN-USB\temperature.c	131;"	f	line:131	signature:(void)
AcquireTemperature	D:\LX-100PIN-USB\temperature.h	44;"	p	line:44	signature:(void)
BD::(ep,dir,pp)((8*ep)+(4*dir))	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	192;"	d	line:192	file:
BD::(ep,dir,pp)(4*(4*ep+2*dir+((ep	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	423;"	d	line:423	file:
BD::(ep,dir,pp)(4*(4*ep+2*dir+pp))	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	346;"	d	line:346	file:
BD::(ep,dir,pp)(4*(ep+dir+(((ep==0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	264;"	d	line:264	file:
BD::(ep,dir,pp)(8*(4*ep+2*dir+pp))	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	348;"	d	line:348	file:
BDT	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	465;"	v	line:465
BDT	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	467;"	v	line:467
BDT	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	469;"	v	line:469
BDT	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	471;"	v	line:471
BaudRateGen	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	123;"	v	line:123
BothEP0OutUOWNsSet	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	446;"	v	line:446
CDCDataInHandle	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	119;"	v	line:119
CDCDataOutHandle	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	118;"	v	line:118
CDCInitEP	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	284;"	f	line:284	signature:(void)
CDCTxService	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	697;"	f	line:697	signature:(void)
CDC_COMM_EP::2	D:\LX-100PIN-USB\usb_config.h	91;"	d	line:91
CDC_COMM_INTF_ID::0x00	D:\LX-100PIN-USB\usb_config.h	90;"	d	line:90
CDC_COMM_IN_EP_SIZE::8	D:\LX-100PIN-USB\usb_config.h	92;"	d	line:92
CDC_DATA_EP::3	D:\LX-100PIN-USB\usb_config.h	94;"	d	line:94
CDC_DATA_INTF_ID::0x01	D:\LX-100PIN-USB\usb_config.h	93;"	d	line:93
CDC_DATA_IN_EP_SIZE::64	D:\LX-100PIN-USB\usb_config.h	95;"	d	line:95
CDC_DATA_OUT_EP_SIZE::64	D:\LX-100PIN-USB\usb_config.h	96;"	d	line:96
CTRL_TRF_RX::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	119;"	d	line:119	file:
CTRL_TRF_TX::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	118;"	d	line:118	file:
CtrlTrfData	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	484;"	v	line:484
DEMO_BOARD::PIC32MX795F512L_PIM	D:\LX-100PIN-USB\HardwareProfile.h	67;"	d	line:67
DelayCnt	D:\LX-100PIN-USB\main.c	73;"	v	line:73
EP0_IN_EVEN::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	127;"	d	line:127	file:
EP0_IN_EVEN::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	359;"	d	line:359	file:
EP0_IN_EVEN::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	200;"	d	line:200	file:
EP0_IN_EVEN::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	280;"	d	line:280	file:
EP0_IN_ODD::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	128;"	d	line:128	file:
EP0_IN_ODD::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	360;"	d	line:360	file:
EP0_IN_ODD::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	201;"	d	line:201	file:
EP0_IN_ODD::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	281;"	d	line:281	file:
EP0_OUT_EVEN::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	125;"	d	line:125	file:
EP0_OUT_EVEN::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	198;"	d	line:198	file:
EP0_OUT_EVEN::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	278;"	d	line:278	file:
EP0_OUT_EVEN::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	357;"	d	line:357	file:
EP0_OUT_ODD::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	126;"	d	line:126	file:
EP0_OUT_ODD::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	358;"	d	line:358	file:
EP0_OUT_ODD::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	199;"	d	line:199	file:
EP0_OUT_ODD::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	279;"	d	line:279	file:
EP10_IN_EVEN::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	167;"	d	line:167	file:
EP10_IN_EVEN::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	240;"	d	line:240	file:
EP10_IN_EVEN::40	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	399;"	d	line:399	file:
EP10_IN_EVEN::42	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	320;"	d	line:320	file:
EP10_IN_ODD::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	168;"	d	line:168	file:
EP10_IN_ODD::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	241;"	d	line:241	file:
EP10_IN_ODD::41	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	400;"	d	line:400	file:
EP10_IN_ODD::43	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	321;"	d	line:321	file:
EP10_OUT_EVEN::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	165;"	d	line:165	file:
EP10_OUT_EVEN::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	238;"	d	line:238	file:
EP10_OUT_EVEN::38	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	397;"	d	line:397	file:
EP10_OUT_EVEN::40	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	318;"	d	line:318	file:
EP10_OUT_ODD::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	166;"	d	line:166	file:
EP10_OUT_ODD::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	239;"	d	line:239	file:
EP10_OUT_ODD::39	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	398;"	d	line:398	file:
EP10_OUT_ODD::41	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	319;"	d	line:319	file:
EP11_IN_EVEN::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	171;"	d	line:171	file:
EP11_IN_EVEN::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	244;"	d	line:244	file:
EP11_IN_EVEN::44	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	403;"	d	line:403	file:
EP11_IN_EVEN::46	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	324;"	d	line:324	file:
EP11_IN_ODD::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	172;"	d	line:172	file:
EP11_IN_ODD::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	245;"	d	line:245	file:
EP11_IN_ODD::45	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	404;"	d	line:404	file:
EP11_IN_ODD::47	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	325;"	d	line:325	file:
EP11_OUT_EVEN::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	169;"	d	line:169	file:
EP11_OUT_EVEN::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	242;"	d	line:242	file:
EP11_OUT_EVEN::42	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	401;"	d	line:401	file:
EP11_OUT_EVEN::44	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	322;"	d	line:322	file:
EP11_OUT_ODD::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	170;"	d	line:170	file:
EP11_OUT_ODD::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	243;"	d	line:243	file:
EP11_OUT_ODD::43	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	402;"	d	line:402	file:
EP11_OUT_ODD::45	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	323;"	d	line:323	file:
EP12_IN_EVEN::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	175;"	d	line:175	file:
EP12_IN_EVEN::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	248;"	d	line:248	file:
EP12_IN_EVEN::48	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	407;"	d	line:407	file:
EP12_IN_EVEN::50	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	328;"	d	line:328	file:
EP12_IN_ODD::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	176;"	d	line:176	file:
EP12_IN_ODD::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	249;"	d	line:249	file:
EP12_IN_ODD::49	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	408;"	d	line:408	file:
EP12_IN_ODD::51	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	329;"	d	line:329	file:
EP12_OUT_EVEN::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	173;"	d	line:173	file:
EP12_OUT_EVEN::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	246;"	d	line:246	file:
EP12_OUT_EVEN::46	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	405;"	d	line:405	file:
EP12_OUT_EVEN::48	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	326;"	d	line:326	file:
EP12_OUT_ODD::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	174;"	d	line:174	file:
EP12_OUT_ODD::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	247;"	d	line:247	file:
EP12_OUT_ODD::47	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	406;"	d	line:406	file:
EP12_OUT_ODD::49	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	327;"	d	line:327	file:
EP13_IN_EVEN::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	179;"	d	line:179	file:
EP13_IN_EVEN::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	252;"	d	line:252	file:
EP13_IN_EVEN::52	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	411;"	d	line:411	file:
EP13_IN_EVEN::54	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	332;"	d	line:332	file:
EP13_IN_ODD::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	180;"	d	line:180	file:
EP13_IN_ODD::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	253;"	d	line:253	file:
EP13_IN_ODD::53	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	412;"	d	line:412	file:
EP13_IN_ODD::55	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	333;"	d	line:333	file:
EP13_OUT_EVEN::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	177;"	d	line:177	file:
EP13_OUT_EVEN::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	250;"	d	line:250	file:
EP13_OUT_EVEN::50	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	409;"	d	line:409	file:
EP13_OUT_EVEN::52	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	330;"	d	line:330	file:
EP13_OUT_ODD::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	178;"	d	line:178	file:
EP13_OUT_ODD::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	251;"	d	line:251	file:
EP13_OUT_ODD::51	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	410;"	d	line:410	file:
EP13_OUT_ODD::53	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	331;"	d	line:331	file:
EP14_IN_EVEN::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	183;"	d	line:183	file:
EP14_IN_EVEN::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	256;"	d	line:256	file:
EP14_IN_EVEN::56	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	415;"	d	line:415	file:
EP14_IN_EVEN::58	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	336;"	d	line:336	file:
EP14_IN_ODD::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	184;"	d	line:184	file:
EP14_IN_ODD::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	257;"	d	line:257	file:
EP14_IN_ODD::57	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	416;"	d	line:416	file:
EP14_IN_ODD::59	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	337;"	d	line:337	file:
EP14_OUT_EVEN::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	181;"	d	line:181	file:
EP14_OUT_EVEN::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	254;"	d	line:254	file:
EP14_OUT_EVEN::54	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	413;"	d	line:413	file:
EP14_OUT_EVEN::56	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	334;"	d	line:334	file:
EP14_OUT_ODD::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	182;"	d	line:182	file:
EP14_OUT_ODD::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	255;"	d	line:255	file:
EP14_OUT_ODD::55	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	414;"	d	line:414	file:
EP14_OUT_ODD::57	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	335;"	d	line:335	file:
EP15_IN_EVEN::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	187;"	d	line:187	file:
EP15_IN_EVEN::32	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	260;"	d	line:260	file:
EP15_IN_EVEN::60	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	419;"	d	line:419	file:
EP15_IN_EVEN::62	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	340;"	d	line:340	file:
EP15_IN_ODD::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	188;"	d	line:188	file:
EP15_IN_ODD::32	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	261;"	d	line:261	file:
EP15_IN_ODD::61	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	420;"	d	line:420	file:
EP15_IN_ODD::63	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	341;"	d	line:341	file:
EP15_OUT_EVEN::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	185;"	d	line:185	file:
EP15_OUT_EVEN::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	258;"	d	line:258	file:
EP15_OUT_EVEN::58	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	417;"	d	line:417	file:
EP15_OUT_EVEN::60	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	338;"	d	line:338	file:
EP15_OUT_ODD::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	186;"	d	line:186	file:
EP15_OUT_ODD::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	259;"	d	line:259	file:
EP15_OUT_ODD::59	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	418;"	d	line:418	file:
EP15_OUT_ODD::61	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	339;"	d	line:339	file:
EP1_IN_EVEN::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	131;"	d	line:131	file:
EP1_IN_EVEN::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	204;"	d	line:204	file:
EP1_IN_EVEN::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	363;"	d	line:363	file:
EP1_IN_EVEN::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	284;"	d	line:284	file:
EP1_IN_ODD::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	132;"	d	line:132	file:
EP1_IN_ODD::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	205;"	d	line:205	file:
EP1_IN_ODD::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	364;"	d	line:364	file:
EP1_IN_ODD::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	285;"	d	line:285	file:
EP1_OUT_EVEN::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	129;"	d	line:129	file:
EP1_OUT_EVEN::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	361;"	d	line:361	file:
EP1_OUT_EVEN::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	202;"	d	line:202	file:
EP1_OUT_EVEN::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	282;"	d	line:282	file:
EP1_OUT_ODD::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	130;"	d	line:130	file:
EP1_OUT_ODD::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	203;"	d	line:203	file:
EP1_OUT_ODD::3	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	362;"	d	line:362	file:
EP1_OUT_ODD::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	283;"	d	line:283	file:
EP2_IN_EVEN::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	288;"	d	line:288	file:
EP2_IN_EVEN::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	135;"	d	line:135	file:
EP2_IN_EVEN::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	208;"	d	line:208	file:
EP2_IN_EVEN::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	367;"	d	line:367	file:
EP2_IN_ODD::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	289;"	d	line:289	file:
EP2_IN_ODD::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	136;"	d	line:136	file:
EP2_IN_ODD::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	209;"	d	line:209	file:
EP2_IN_ODD::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	368;"	d	line:368	file:
EP2_OUT_EVEN::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	133;"	d	line:133	file:
EP2_OUT_EVEN::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	206;"	d	line:206	file:
EP2_OUT_EVEN::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	365;"	d	line:365	file:
EP2_OUT_EVEN::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	286;"	d	line:286	file:
EP2_OUT_ODD::4	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	134;"	d	line:134	file:
EP2_OUT_ODD::5	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	207;"	d	line:207	file:
EP2_OUT_ODD::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	366;"	d	line:366	file:
EP2_OUT_ODD::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	287;"	d	line:287	file:
EP3_IN_EVEN::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	371;"	d	line:371	file:
EP3_IN_EVEN::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	292;"	d	line:292	file:
EP3_IN_EVEN::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	139;"	d	line:139	file:
EP3_IN_EVEN::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	212;"	d	line:212	file:
EP3_IN_ODD::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	372;"	d	line:372	file:
EP3_IN_ODD::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	293;"	d	line:293	file:
EP3_IN_ODD::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	140;"	d	line:140	file:
EP3_IN_ODD::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	213;"	d	line:213	file:
EP3_OUT_EVEN::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	369;"	d	line:369	file:
EP3_OUT_EVEN::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	290;"	d	line:290	file:
EP3_OUT_EVEN::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	137;"	d	line:137	file:
EP3_OUT_EVEN::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	210;"	d	line:210	file:
EP3_OUT_ODD::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	370;"	d	line:370	file:
EP3_OUT_ODD::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	291;"	d	line:291	file:
EP3_OUT_ODD::6	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	138;"	d	line:138	file:
EP3_OUT_ODD::7	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	211;"	d	line:211	file:
EP4_IN_EVEN::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	216;"	d	line:216	file:
EP4_IN_EVEN::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	375;"	d	line:375	file:
EP4_IN_EVEN::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	296;"	d	line:296	file:
EP4_IN_EVEN::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	143;"	d	line:143	file:
EP4_IN_ODD::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	217;"	d	line:217	file:
EP4_IN_ODD::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	376;"	d	line:376	file:
EP4_IN_ODD::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	297;"	d	line:297	file:
EP4_IN_ODD::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	144;"	d	line:144	file:
EP4_OUT_EVEN::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	373;"	d	line:373	file:
EP4_OUT_EVEN::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	294;"	d	line:294	file:
EP4_OUT_EVEN::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	141;"	d	line:141	file:
EP4_OUT_EVEN::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	214;"	d	line:214	file:
EP4_OUT_ODD::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	374;"	d	line:374	file:
EP4_OUT_ODD::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	295;"	d	line:295	file:
EP4_OUT_ODD::8	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	142;"	d	line:142	file:
EP4_OUT_ODD::9	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	215;"	d	line:215	file:
EP5_IN_EVEN::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	147;"	d	line:147	file:
EP5_IN_EVEN::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	220;"	d	line:220	file:
EP5_IN_EVEN::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	379;"	d	line:379	file:
EP5_IN_EVEN::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	300;"	d	line:300	file:
EP5_IN_ODD::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	148;"	d	line:148	file:
EP5_IN_ODD::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	221;"	d	line:221	file:
EP5_IN_ODD::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	380;"	d	line:380	file:
EP5_IN_ODD::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	301;"	d	line:301	file:
EP5_OUT_EVEN::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	145;"	d	line:145	file:
EP5_OUT_EVEN::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	218;"	d	line:218	file:
EP5_OUT_EVEN::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	377;"	d	line:377	file:
EP5_OUT_EVEN::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	298;"	d	line:298	file:
EP5_OUT_ODD::10	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	146;"	d	line:146	file:
EP5_OUT_ODD::11	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	219;"	d	line:219	file:
EP5_OUT_ODD::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	378;"	d	line:378	file:
EP5_OUT_ODD::21	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	299;"	d	line:299	file:
EP6_IN_EVEN::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	151;"	d	line:151	file:
EP6_IN_EVEN::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	224;"	d	line:224	file:
EP6_IN_EVEN::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	383;"	d	line:383	file:
EP6_IN_EVEN::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	304;"	d	line:304	file:
EP6_IN_ODD::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	152;"	d	line:152	file:
EP6_IN_ODD::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	225;"	d	line:225	file:
EP6_IN_ODD::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	384;"	d	line:384	file:
EP6_IN_ODD::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	305;"	d	line:305	file:
EP6_OUT_EVEN::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	149;"	d	line:149	file:
EP6_OUT_EVEN::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	222;"	d	line:222	file:
EP6_OUT_EVEN::22	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	381;"	d	line:381	file:
EP6_OUT_EVEN::24	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	302;"	d	line:302	file:
EP6_OUT_ODD::12	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	150;"	d	line:150	file:
EP6_OUT_ODD::13	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	223;"	d	line:223	file:
EP6_OUT_ODD::23	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	382;"	d	line:382	file:
EP6_OUT_ODD::25	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	303;"	d	line:303	file:
EP7_IN_EVEN::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	155;"	d	line:155	file:
EP7_IN_EVEN::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	228;"	d	line:228	file:
EP7_IN_EVEN::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	387;"	d	line:387	file:
EP7_IN_EVEN::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	308;"	d	line:308	file:
EP7_IN_ODD::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	156;"	d	line:156	file:
EP7_IN_ODD::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	229;"	d	line:229	file:
EP7_IN_ODD::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	388;"	d	line:388	file:
EP7_IN_ODD::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	309;"	d	line:309	file:
EP7_OUT_EVEN::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	153;"	d	line:153	file:
EP7_OUT_EVEN::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	226;"	d	line:226	file:
EP7_OUT_EVEN::26	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	385;"	d	line:385	file:
EP7_OUT_EVEN::28	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	306;"	d	line:306	file:
EP7_OUT_ODD::14	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	154;"	d	line:154	file:
EP7_OUT_ODD::15	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	227;"	d	line:227	file:
EP7_OUT_ODD::27	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	386;"	d	line:386	file:
EP7_OUT_ODD::29	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	307;"	d	line:307	file:
EP8_IN_EVEN::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	159;"	d	line:159	file:
EP8_IN_EVEN::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	232;"	d	line:232	file:
EP8_IN_EVEN::32	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	391;"	d	line:391	file:
EP8_IN_EVEN::34	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	312;"	d	line:312	file:
EP8_IN_ODD::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	160;"	d	line:160	file:
EP8_IN_ODD::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	233;"	d	line:233	file:
EP8_IN_ODD::33	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	392;"	d	line:392	file:
EP8_IN_ODD::35	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	313;"	d	line:313	file:
EP8_OUT_EVEN::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	157;"	d	line:157	file:
EP8_OUT_EVEN::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	230;"	d	line:230	file:
EP8_OUT_EVEN::30	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	389;"	d	line:389	file:
EP8_OUT_EVEN::32	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	310;"	d	line:310	file:
EP8_OUT_ODD::16	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	158;"	d	line:158	file:
EP8_OUT_ODD::17	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	231;"	d	line:231	file:
EP8_OUT_ODD::31	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	390;"	d	line:390	file:
EP8_OUT_ODD::33	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	311;"	d	line:311	file:
EP9_IN_EVEN::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	163;"	d	line:163	file:
EP9_IN_EVEN::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	236;"	d	line:236	file:
EP9_IN_EVEN::36	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	395;"	d	line:395	file:
EP9_IN_EVEN::38	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	316;"	d	line:316	file:
EP9_IN_ODD::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	164;"	d	line:164	file:
EP9_IN_ODD::20	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	237;"	d	line:237	file:
EP9_IN_ODD::37	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	396;"	d	line:396	file:
EP9_IN_ODD::39	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	317;"	d	line:317	file:
EP9_OUT_EVEN::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	161;"	d	line:161	file:
EP9_OUT_EVEN::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	234;"	d	line:234	file:
EP9_OUT_EVEN::34	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	393;"	d	line:393	file:
EP9_OUT_EVEN::36	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	314;"	d	line:314	file:
EP9_OUT_ODD::18	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	162;"	d	line:162	file:
EP9_OUT_ODD::19	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	235;"	d	line:235	file:
EP9_OUT_ODD::35	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	394;"	d	line:394	file:
EP9_OUT_ODD::37	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	315;"	d	line:315	file:
EP::(ep,dir,pp)(2*ep+dir)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	190;"	d	line:190	file:
EP::(ep,dir,pp)(2*ep+dir+(((ep==0)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	263;"	d	line:263	file:
EP::(ep,dir,pp)(4*ep+2*dir+((ep==0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	422;"	d	line:422	file:
EP::(ep,dir,pp)(4*ep+2*dir+pp)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	343;"	d	line:343	file:
EXPLORER_16	D:\LX-100PIN-USB\HardwareProfile.h	68;"	d	line:68
HARDWARE_PROFILE_H	D:\LX-100PIN-USB\HardwareProfile.h	48;"	d	line:48
INPUT_PIN::1	D:\LX-100PIN-USB\HardwareProfile.h	112;"	d	line:112
InitTempSensor	D:\LX-100PIN-USB\temperature.c	73;"	f	line:73	signature:(void)
InitTempSensor	D:\LX-100PIN-USB\temperature.h	43;"	p	line:43	signature:(void)
InitializeSystem	D:\LX-100PIN-USB\main.c	144;"	f	line:144	file:	signature:(void)
InitializeSystem	D:\LX-100PIN-USB\main.c	76;"	p	line:76	file:	signature:(void)
MY_PID::0x000A	D:\LX-100PIN-USB\usb_config.h	62;"	d	line:62
MY_VID::0x04D8	D:\LX-100PIN-USB\usb_config.h	61;"	d	line:61
OUTPUT_PIN::0	D:\LX-100PIN-USB\HardwareProfile.h	113;"	d	line:113
PIC32MX795F512L_PIM	D:\LX-100PIN-USB\HardwareProfile.h	69;"	d	line:69
ProcessIO	D:\LX-100PIN-USB\main.c	237;"	f	line:237	signature:(void)
ProcessIO	D:\LX-100PIN-USB\main.c	77;"	p	line:77	file:	signature:(void)
RemoteWakeup	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	444;"	v	line:444
SHORT_PKT_NOT_USED::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	112;"	d	line:112	file:
SHORT_PKT_PENDING::1	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	113;"	d	line:113	file:
SHORT_PKT_SENT::2	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	114;"	d	line:114	file:
SetupPkt	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	483;"	v	line:483
SwitchIsPressed	D:\LX-100PIN-USB\temperature.c	203;"	f	line:203	signature:(void)
SwitchIsPressed	D:\LX-100PIN-USB\temperature.h	46;"	p	line:46	signature:(void)
TEMPERATURE_H	D:\LX-100PIN-USB\temperature.h	35;"	d	line:35
USBActiveConfiguration	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	433;"	v	line:433
USBAlternateInterface	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	434;"	v	line:434
USBCDCSetLineCoding	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	141;"	p	line:141	file:	signature:(void)
USBCancelIO	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2528;"	f	line:2528	signature:(BYTE endpoint)
USBCheckCDCRequest	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	168;"	f	line:168	signature:(void)
USBCheckStdRequest	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1533;"	f	line:1533	signature:(void)
USBCheckStdRequest	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	599;"	p	line:599	file:	signature:(void)
USBConfigureEndpoint	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2271;"	f	line:2271	signature:(BYTE EPNum, BYTE direction)
USBConfigureEndpoint	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	612;"	p	line:612	file:	signature:(BYTE EPNum, BYTE direction)
USBCtrlEPService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1224;"	f	line:1224	signature:(void)
USBCtrlEPService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	596;"	p	line:596	file:	signature:(void)
USBCtrlEPServiceComplete	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1884;"	f	line:1884	signature:(void)
USBCtrlEPServiceComplete	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	601;"	p	line:601	file:	signature:(void)
USBCtrlTrfInHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1415;"	f	line:1415	signature:(void)
USBCtrlTrfInHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	598;"	p	line:598	file:	signature:(void)
USBCtrlTrfOutHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1365;"	f	line:1365	signature:(void)
USBCtrlTrfOutHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	608;"	p	line:608	file:	signature:(void)
USBCtrlTrfRxService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2126;"	f	line:2126	signature:(void)
USBCtrlTrfRxService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	604;"	p	line:604	file:	signature:(void)
USBCtrlTrfSetupHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1318;"	f	line:1318	signature:(void)
USBCtrlTrfSetupHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	597;"	p	line:597	file:	signature:(void)
USBCtrlTrfTxService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2031;"	f	line:2031	signature:(void)
USBCtrlTrfTxService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	602;"	p	line:602	file:	signature:(void)
USBDeviceAttach	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2660;"	f	line:2660	signature:(void)
USBDeviceDetach	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2569;"	f	line:2569	signature:(void)
USBDeviceInit	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	645;"	f	line:645	signature:(void)
USBDeviceState	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	432;"	v	line:432
USBDeviceTasks	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	742;"	f	line:742	signature:(void)
USBEPService	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	611;"	p	line:611	file:	signature:(void)
USBEnableEndpoint	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2359;"	f	line:2359	signature:(BYTE ep, BYTE options)
USBEnableEndpoint	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	619;"	p	line:619	file:	signature:(BYTE ep,BYTE options)
USBInData	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	448;"	v	line:448
USBInMaxPacketSize	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	447;"	v	line:447
USBIsTxBusy	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	609;"	p	line:609	file:	signature:(BYTE EPNumber)
USBPrepareForNextSetupTrf	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1487;"	f	line:1487	signature:(void)
USBPrepareForNextSetupTrf	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	603;"	p	line:603	file:	signature:(void)
USBProtocolResetHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	614;"	p	line:614	file:	signature:(void)
USBPut	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	610;"	p	line:610	file:	signature:(BYTE EPNum, BYTE Data)
USBStallEndpoint	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2401;"	f	line:2401	signature:(BYTE ep, BYTE dir)
USBStallHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1059;"	f	line:1059	signature:(void)
USBStallHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	617;"	p	line:617	file:	signature:(void)
USBStdFeatureReqHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1598;"	f	line:1598	signature:(void)
USBStdFeatureReqHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	607;"	p	line:607	file:	signature:(void)
USBStdGetDscHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1737;"	f	line:1737	signature:(void)
USBStdGetDscHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	600;"	p	line:600	file:	signature:(void)
USBStdGetStatusHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1799;"	f	line:1799	signature:(void)
USBStdGetStatusHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	606;"	p	line:606	file:	signature:(void)
USBStdSetCfgHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2204;"	f	line:2204	signature:(void)
USBStdSetCfgHandler	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	605;"	p	line:605	file:	signature:(void)
USBSuspend	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1102;"	f	line:1102	signature:(void)
USBSuspend	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	616;"	p	line:616	file:	signature:(void)
USBTransferOnePacket	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2459;"	f	line:2459	signature:(BYTE ep,BYTE dir,BYTE* data,BYTE len)
USBTransferOnePacket	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	618;"	p	line:618	file:	signature:(BYTE ep, BYTE dir, BYTE* data, BYTE len)
USBWakeFromSuspend	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1159;"	f	line:1159	signature:(void)
USBWakeFromSuspend	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	615;"	p	line:615	file:	signature:(void)
USB_BUS_SENSE::0	D:\LX-100PIN-USB\HardwareProfile.h	57;"	d	line:57
USB_CDC_SET_LINE_CODING_HANDLER	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	137;"	p	line:137	file:
USB_CDC_SUPPORT_ABSTRACT_CONTROL_MANAGEMENT_CAPABILITIES_D1::	D:\LX-100PIN-USB\usb_config.h	99;"	d	line:99
USB_CD_Ptr	D:\LX-100PIN-USB\usb_descriptors.c	294;"	v	line:294
USB_DISABLE_NONSTANDARD_EP0_REQUEST_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	567;"	d	line:567	file:
USB_DISABLE_NONSTANDARD_EP0_REQUEST_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	569;"	d	line:569	file:
USB_ENABLE_ALL_HANDLERS	D:\LX-100PIN-USB\usb_config.h	72;"	d	line:72
USB_EP0_BUFF_SIZE::8	D:\LX-100PIN-USB\usb_config.h	67;"	d	line:67
USB_ERROR_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	561;"	d	line:561	file:
USB_ERROR_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	563;"	d	line:563	file:
USB_INTERRUPT	D:\LX-100PIN-USB\usb_config.h	64;"	d	line:64
USB_In_Buffer	D:\LX-100PIN-USB\main.c	71;"	v	line:71
USB_MAX_EP_NUMBER::3	D:\LX-100PIN-USB\usb_config.h	69;"	d	line:69
USB_MAX_NUM_INT::(0+1)	D:\LX-100PIN-USB\usb_config.h	68;"	d	line:68
USB_NEXT_EP0_IN_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	123;"	d	line:123	file:
USB_NEXT_EP0_IN_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	196;"	d	line:196	file:
USB_NEXT_EP0_IN_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	355;"	d	line:355	file:
USB_NEXT_EP0_IN_PING_PONG::0x0004	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	269;"	d	line:269	file:
USB_NEXT_EP0_IN_PING_PONG::0x0008	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	273;"	d	line:273	file:
USB_NEXT_EP0_OUT_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	122;"	d	line:122	file:
USB_NEXT_EP0_OUT_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	354;"	d	line:354	file:
USB_NEXT_EP0_OUT_PING_PONG::0x0004	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	195;"	d	line:195	file:
USB_NEXT_EP0_OUT_PING_PONG::0x0004	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	268;"	d	line:268	file:
USB_NEXT_EP0_OUT_PING_PONG::0x0008	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	272;"	d	line:272	file:
USB_NEXT_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	124;"	d	line:124	file:
USB_NEXT_PING_PONG::0x0000	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	197;"	d	line:197	file:
USB_NEXT_PING_PONG::0x0004	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	270;"	d	line:270	file:
USB_NEXT_PING_PONG::0x0004	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	356;"	d	line:356	file:
USB_NEXT_PING_PONG::0x0008	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	274;"	d	line:274	file:
USB_NUM_STRING_DESCRIPTORS::3	D:\LX-100PIN-USB\usb_config.h	70;"	d	line:70
USB_Out_Buffer	D:\LX-100PIN-USB\main.c	70;"	v	line:70
USB_PING_PONG_MODE::USB_PING_PONG__FULL_PING_PONG	D:\LX-100PIN-USB\usb_config.h	57;"	d	line:57
USB_PULLUP_OPTION::USB_PULLUP_ENABLE	D:\LX-100PIN-USB\usb_config.h	65;"	d	line:65
USB_SD_Ptr	D:\LX-100PIN-USB\usb_descriptors.c	299;"	v	line:299
USB_SET_CONFIGURATION_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	579;"	d	line:579	file:
USB_SET_CONFIGURATION_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	581;"	d	line:581	file:
USB_SET_DESCRIPTOR_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	573;"	d	line:573	file:
USB_SET_DESCRIPTOR_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	575;"	d	line:575	file:
USB_SOF_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	555;"	d	line:555	file:
USB_SOF_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	557;"	d	line:557	file:
USB_SPEED_OPTION::USB_FULL_SPEED	D:\LX-100PIN-USB\usb_config.h	63;"	d	line:63
USB_SUPPORT_DEVICE	D:\LX-100PIN-USB\usb_config.h	53;"	d	line:53
USB_SUSPEND_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	539;"	d	line:539	file:
USB_SUSPEND_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	543;"	d	line:543	file:
USB_TRANSCEIVER_OPTION::USB_INTERNAL_TRANSCEIVER	D:\LX-100PIN-USB\usb_config.h	66;"	d	line:66
USB_TRASFER_COMPLETE_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	585;"	d	line:585	file:
USB_TRASFER_COMPLETE_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	587;"	d	line:587	file:
USB_USER_CONFIG_DESCRIPTOR::USB_CD_Ptr	D:\LX-100PIN-USB\usb_config.h	84;"	d	line:84
USB_USER_CONFIG_DESCRIPTOR_INCLUDE::externROMBYTE*ROMUSB_CD_Ptr[]	D:\LX-100PIN-USB\usb_config.h	85;"	d	line:85
USB_USER_DEVICE_DESCRIPTOR::&device_dsc	D:\LX-100PIN-USB\usb_config.h	82;"	d	line:82
USB_USER_DEVICE_DESCRIPTOR_INCLUDE::externROMUSB_DEVICE_DESCRIPTOR	D:\LX-100PIN-USB\usb_config.h	83;"	d	line:83
USB_USE_CDC	D:\LX-100PIN-USB\usb_config.h	89;"	d	line:89
USB_WAKEUP_FROM_SUSPEND_HANDLER::(event,pointer,size)	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	547;"	d	line:547	file:
USB_WAKEUP_FROM_SUSPEND_HANDLER::(event,pointer,size)USER_USB_C	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	551;"	d	line:551	file:
USER_USB_CALLBACK_EVENT_HANDLER	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	593;"	p	line:593	file:	signature:(USB_EVENT event, void *pdata, WORD size)
USER_USB_CALLBACK_EVENT_HANDLER	D:\LX-100PIN-USB\main.c	279;"	f	line:279	signature:(USB_EVENT event, void *pdata, WORD size)
USTATcopy	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	445;"	v	line:445
UpdateCelsiusASCII	D:\LX-100PIN-USB\temperature.c	162;"	f	line:162	signature:(void)
UpdateCelsiusASCII	D:\LX-100PIN-USB\temperature.h	45;"	p	line:45	signature:(void)
UserInit	D:\LX-100PIN-USB\main.c	211;"	f	line:211	signature:(void)
UserInit	D:\LX-100PIN-USB\main.c	78;"	p	line:78	file:	signature:(void)
WAIT_SETUP::0	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	117;"	d	line:117	file:
_USB_CONFIG_VERSION_BUILD::0	D:\LX-100PIN-USB\usb_config.h	49;"	d	line:49
_USB_CONFIG_VERSION_DOT::0	D:\LX-100PIN-USB\usb_config.h	48;"	d	line:48
_USB_CONFIG_VERSION_MAJOR::2	D:\LX-100PIN-USB\usb_config.h	46;"	d	line:46
_USB_CONFIG_VERSION_MINOR::5	D:\LX-100PIN-USB\usb_config.h	47;"	d	line:47
__USB_DESCRIPTORS_C	D:\LX-100PIN-USB\usb_descriptors.c	154;"	d	line:154	file:
_usb_config_h_	D:\LX-100PIN-USB\usb_config.h	33;"	d	line:33
bDscType	D:\LX-100PIN-USB\usb_descriptors.c	275;"	m	line:275	file:
bDscType	D:\LX-100PIN-USB\usb_descriptors.c	279;"	m	line:279	file:
bDscType	D:\LX-100PIN-USB\usb_descriptors.c	287;"	m	line:287	file:
bLength	D:\LX-100PIN-USB\usb_descriptors.c	275;"	m	line:275	file:
bLength	D:\LX-100PIN-USB\usb_descriptors.c	279;"	m	line:279	file:
bLength	D:\LX-100PIN-USB\usb_descriptors.c	287;"	m	line:287	file:
byteToRead	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2128;"	l	line:2128
byteToSend	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2033;"	l	line:2033
byte_to_send	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	699;"	l	line:699
cdc_data_rx	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	105;"	v	line:105
cdc_data_tx	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	106;"	v	line:106
cdc_mem_type	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	116;"	v	line:116
cdc_notice	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	104;"	v	line:104
cdc_rx_len	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	110;"	v	line:110
cdc_trf_state	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	112;"	v	line:112
cdc_tx_len	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	115;"	v	line:115
configDescriptor1	D:\LX-100PIN-USB\usb_descriptors.c	186;"	v	line:186
controlTransferState	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	440;"	v	line:440
control_signal_bitmap	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	122;"	v	line:122
counter	D:\LX-100PIN-USB\temperature.c	134;"	l	line:134
device_dsc	D:\LX-100PIN-USB\usb_descriptors.c	167;"	v	line:167
dummy_encapsulated_cmd_response	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	134;"	v	line:134
dummy_length::0x08	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	133;"	d	line:133	file:
getsUSBUSART	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	352;"	f	line:352	signature:(char *buffer, BYTE len)
handle	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2273;"	l	line:2273
handle	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2461;"	l	line:2461
hid_report_in	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	492;"	v	line:492
hid_report_out	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	491;"	v	line:491
i	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	700;"	l	line:700
i	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2129;"	l	line:2129
i	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2206;"	l	line:2206
i	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	647;"	l	line:647
i	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	754;"	l	line:754
inPipes	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	441;"	v	line:441
lastDTS	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1417;"	l	line:1417
len	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	498;"	l	line:498
len	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	595;"	l	line:595
line_coding	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	107;"	v	line:107
mGetLED_1::mLED_1	D:\LX-100PIN-USB\HardwareProfile.h	91;"	d	line:91
mGetLED_2::mLED_2	D:\LX-100PIN-USB\HardwareProfile.h	92;"	d	line:92
mGetLED_3::mLED_3	D:\LX-100PIN-USB\HardwareProfile.h	93;"	d	line:93
mGetLED_4::mLED_4	D:\LX-100PIN-USB\HardwareProfile.h	94;"	d	line:94
mInitAllLEDs::LATE&=0xFF00;TRISE&=0xFF00;	D:\LX-100PIN-USB\HardwareProfile.h	72;"	d	line:72
mInitAllSwitches::mInitSwitch3;mInitSwitch4;mIni	D:\LX-100PIN-USB\HardwareProfile.h	84;"	d	line:84
mInitSwitch3::TRISBbits.TRISB2=1;	D:\LX-100PIN-USB\HardwareProfile.h	80;"	d	line:80
mInitSwitch4::TRISBbits.TRISB3=1;	D:\LX-100PIN-USB\HardwareProfile.h	81;"	d	line:81
mInitSwitch5::TRISBbits.TRISB6=1;	D:\LX-100PIN-USB\HardwareProfile.h	82;"	d	line:82
mInitSwitch6::TRISBbits.TRISB7=1;	D:\LX-100PIN-USB\HardwareProfile.h	83;"	d	line:83
mLED_1::LATEbits.LATE0	D:\LX-100PIN-USB\HardwareProfile.h	74;"	d	line:74
mLED_1_Off::mLED_1=0;	D:\LX-100PIN-USB\HardwareProfile.h	99;"	d	line:99
mLED_1_On::mLED_1=1;	D:\LX-100PIN-USB\HardwareProfile.h	95;"	d	line:95
mLED_1_Toggle::mLED_1=!mLED_1;	D:\LX-100PIN-USB\HardwareProfile.h	103;"	d	line:103
mLED_2::LATEbits.LATE1	D:\LX-100PIN-USB\HardwareProfile.h	75;"	d	line:75
mLED_2_Off::mLED_2=0;	D:\LX-100PIN-USB\HardwareProfile.h	100;"	d	line:100
mLED_2_On::mLED_2=1;	D:\LX-100PIN-USB\HardwareProfile.h	96;"	d	line:96
mLED_2_Toggle::mLED_2=!mLED_2;	D:\LX-100PIN-USB\HardwareProfile.h	104;"	d	line:104
mLED_3::LATEbits.LATE2	D:\LX-100PIN-USB\HardwareProfile.h	76;"	d	line:76
mLED_3_Off::mLED_3=0;	D:\LX-100PIN-USB\HardwareProfile.h	101;"	d	line:101
mLED_3_On::mLED_3=1;	D:\LX-100PIN-USB\HardwareProfile.h	97;"	d	line:97
mLED_3_Toggle::mLED_3=!mLED_3;	D:\LX-100PIN-USB\HardwareProfile.h	105;"	d	line:105
mLED_4::LATEbits.LATE3	D:\LX-100PIN-USB\HardwareProfile.h	77;"	d	line:77
mLED_4_Off::mLED_4=0;	D:\LX-100PIN-USB\HardwareProfile.h	102;"	d	line:102
mLED_4_On::mLED_4=1;	D:\LX-100PIN-USB\HardwareProfile.h	98;"	d	line:98
mLED_4_Toggle::mLED_4=!mLED_4;	D:\LX-100PIN-USB\HardwareProfile.h	106;"	d	line:106
main	D:\LX-100PIN-USB\main.c	99;"	f	line:99	signature:(void)
msd_buffer	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	504;"	v	line:504
msd_cbw	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	497;"	v	line:497
msd_csw	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	498;"	v	line:498
old_sw	D:\LX-100PIN-USB\temperature.c	50;"	v	line:50
outPipes	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	442;"	v	line:442
p	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1498;"	l	line:1498
p	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1600;"	l	line:1600
p	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1831;"	l	line:1831
p	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2364;"	l	line:2364
p	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2403;"	l	line:2403
pBDTEntryEP0OutCurrent	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	435;"	v	line:435
pBDTEntryEP0OutNext	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	436;"	v	line:436
pBDTEntryIn	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	438;"	v	line:438
pBDTEntryOut	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	437;"	v	line:437
pCDCDst	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	114;"	v	line:114
pCDCSrc	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	113;"	v	line:113
pData	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	499;"	l	line:499
pData	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	596;"	l	line:596
pDst	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	443;"	v	line:443
pFunc	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1511;"	p	line:1511	file:
pFunc	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	2180;"	p	line:2180	file:
pUEP	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1602;"	l	line:1602
pUEP	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1604;"	l	line:1604
putUSBUSART	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	423;"	f	line:423	signature:(char *data, BYTE length)
putrsUSBUSART	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	593;"	f	line:593	signature:(const ROM char *data)
putsUSBUSART	D:\LX-100PIN-USB\Microchip\USB\CDC Device Driver\usb_function_cdc.c	496;"	f	line:496	signature:(char *data)
sd000	D:\LX-100PIN-USB\usb_descriptors.c	275;"	v	line:275
sd001	D:\LX-100PIN-USB\usb_descriptors.c	279;"	v	line:279
sd002	D:\LX-100PIN-USB\usb_descriptors.c	287;"	v	line:287
self_power::1	D:\LX-100PIN-USB\HardwareProfile.h	53;"	d	line:53
setup_cnt	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	1251;"	l	line:1251
shortPacketStatus	D:\LX-100PIN-USB\Microchip\USB\usb_device.c	439;"	v	line:439
string	D:\LX-100PIN-USB\usb_descriptors.c	275;"	m	line:275	file:
string	D:\LX-100PIN-USB\usb_descriptors.c	279;"	m	line:279	file:
string	D:\LX-100PIN-USB\usb_descriptors.c	287;"	m	line:287	file:
sw3::PORTBbits.RB2	D:\LX-100PIN-USB\HardwareProfile.h	85;"	d	line:85
sw4::PORTBbits.RB3	D:\LX-100PIN-USB\HardwareProfile.h	86;"	d	line:86
sw5::PORTBbits.RB6	D:\LX-100PIN-USB\HardwareProfile.h	87;"	d	line:87
sw6::PORTBbits.RB7	D:\LX-100PIN-USB\HardwareProfile.h	88;"	d	line:88
sw::sw3	D:\LX-100PIN-USB\HardwareProfile.h	109;"	d	line:109
temp	D:\LX-100PIN-USB\temperature.c	133;"	l	line:133
temp	D:\LX-100PIN-USB\temperature.c	164;"	l	line:164
tempString	D:\LX-100PIN-USB\temperature.c	52;"	v	line:52
temperature	D:\LX-100PIN-USB\temperature.c	51;"	v	line:51
tris_self_power::TRISAbits.TRISA2	D:\LX-100PIN-USB\HardwareProfile.h	52;"	d	line:52
tris_usb_bus_sense::TRISBbits.TRISB0	D:\LX-100PIN-USB\HardwareProfile.h	56;"	d	line:56
